ASSIGNMENT-3

TEAM ID : PNT2022TMID42646

TEAM MEMBER: DANIEL JAYASURYA E(711119106006)

EMAIL ID : danielsurya0108@gmail.com

1.**PYTHON CODE FOR BLINKING LED FOR RASPBERRY PI.**

import RPi.GPIO as GPIO

import time

#assign numbering for the GPIO using BCM

GPIO.setmode(GPIO.BCM)

#assingn number for the GPIO using Board

#GPIO.setmode(GPIO.BOARD)

cnt = 0

MAIL\_CHECK\_FREQ = 1 # change LED status every 1 seconds

RED\_LED = 4

GPIO.setup(RED\_LED, GPIO.OUT)

while True:

ifcnt == 0 :

GPIO.output(RED\_LED, False)

cnt = 1

else:

GPIO.output(RED\_LED, True)

cnt = 0

time.sleep(MAIL\_CHECK\_FREQ)

GPIO.cleanup()

**2.PYTHON CODE FOR TRAFFIC LIGHTS FOR RASPBERRY PI**

import RPi.GPIO as GPIO

import time

try:

def lightTraffic(led1, led2, led3, delay):

GPIO.output(led1, 1)

time.sleep(delay)

GPIO.output(led1, 0)

GPIO.output(led2, 1)

time.sleep(delay)

GPIO.output(led2, 0)

GPIO.output(led3, 1)

time.sleep(delay)

GPIO.output(led3, 0)

GPIO.setmode(GPIO.BCM)

button = 19

GPIO.setup(button, GPIO.IN, pull\_up\_down=GPIO.PUD\_UP)

ledGreen = 16

ledYellow = 12

ledRed = 23

GPIO.setup(ledGreen, GPIO.OUT)

GPIO.setup(ledYellow, GPIO.OUT)

GPIO.setup(ledRed, GPIO.OUT)

while True:

input\_state = GPIO.input(button)

if input\_state == False:

print('Button Pressed')

lightTraffic(ledGreen, ledYellow, ledRed, 1)

else:

GPIO.output(ledGreen, 0)

GPIO.output(ledYellow, 0)

GPIO.output(ledRed, 0)

except KeyboardInterrupt:

print

"You've exited the program"

finally:

GPIO.cleanup()